

**CN LAB 5**

**Configure http and DNS server**

1.End Device PC and a server




2.Go to server



3.Edit index.html


Server->Services->index.html->edit



4.Go to end device.


->Desktop->Web Browser

Type [www.cnlab.com](http://www.cnlab.com) ->Go




**Configure DHCP within a LAN**

1. Two end devices, a switch , router and a Server.




1. Configure ip addres pf router using CLI
2. Configure ip address of server using Server->Desktop->IP Configuration




1. Server->Services


Set the pool name, default gateway=IP address of the router, TFTP Server=IP address of the Server



1. The ip address of the end devices gets assigned automatically


Goto PC0->Desktop->IP Configuration->select DHCP{IPv4}






**Configure DHCP outside a LAN**


1. Two end devices, a switch, router and a server.



1. Router CLI



1. Server->Services



1. End devices

